
     XRouter Version 504e (all variants) - Changes Since V504c
     =========================================================

v504d:

- Fixed:  Occasional segfault on incoming TCP connections, only on
          64-bit versions using XRouter's IP stack.


V504e:

- Fixed:  Setting a port's IPLINK to 255.255.255.255 caused XR to crash
          after receiving nodes broadcast from a peer.

- Fixed:  Nodes broadcasts were not being sent to peers in Ad-Hoc
          networking mode (i.e. IPLINK=0.0.0.0).

- Fixed:  In Ad-Hoc-Networking (AHN) mode, PEER addresses only worked
          if they were IP addresses, i.e. hostnames wouldn't work.

- Fixed:  Minor format error in caption for "Nodes Matching .."

- Change: Better error reporting for SEND and CQ commands.

- Change: In an attempt to reduce confusion, RESTART now re-starts the
          existing copy of Xrouter, whatever its name, while the
          previously-disabled REBOOT command now loads a fresh copy of
          "xrpi", "xrlin", or "xrwin.exe".

          Use RESTART to re-start after a configuration change, or
          REBOOT to load a new version.  Or just Alt-X and start xrouter
          in the usual way.  REBOOT probably won't work properly if you
          are running XRouter as a daemon or service.

