{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Cart"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Cart","index":0,"n_rows":18,"n_cols":4,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Mfr part number","Quantity","Customer part no.","Description"]
["667-ECA-1CM470I ",1,"C1","5mm Diameter, 2.5mm Pitch"]
["594-K104K20X7RH5UH5",3,"C2,C3,C4","5mm Diameter, 2.5mm Pitch"]
["512-1N4148 ",1,"D2","DO-35 "]
["485-2222",1,"J2","2x20 Female GPIO Header"]
["223-CON-SMA-EDGE",1,"J4","SMA Edge mount"]
["623-5943000201 ",1,"L1","FT37-43 Toroid"]
["859-LTL-4291N",1,"D1","LED"]
["512-BS170",1,"Q1","TO-92"]
["531-PT6KV-20K",1,"RV1","20K POT"]
["708-CFM12JT47R0 ",1,"R2","Carbon Film Resistors - Through Hole 47ohm 5% 1/2W Carbon Film"]
["603-CFR-25JT-52-20K ",1,"R3","Carbon Film Resistors - Through Hole 20K ohm 5%"]
["660-CF1/4CT52A1R0J ",1,"R4","Carbon Film Resistors - Through Hole 1ohm 5%"]
["660-CF1/4CT52R153J ",1,"R5","Carbon Film Resistors - Through Hole 15K ohm 5%"]
["660-CF1/4C271J ",1,"R6","Carbon Film Resistors - Through Hole 270 ohm 5%"]
["660-CF1/4CT52R202J ",1,"R7","Carbon Film Resistors - Through Hole 2K ohm 5%"]
["706-95C06B3T",1,"SW1","6mm Push Button Switch"]
["649-1012937890402BLF ",2,"H1","4x1 2.54mm headers"]